System Server Report

# Summary

Total HMC Systems: 1  
Total System Servers: 3  
Total LPARs: 9

# HMC Information

|  |  |
| --- | --- |
| Hostname | AABASMC2 |
| Model | 7063-CR2 |
| Serial | 78A344D |
| Base Version | V10R3 |
| Service Pack | 1060 |
| Gateway | 172.24.193.49 |
| Ip Addr - Eth0 | 172.24.193.7/255.255.255.224 |
| Ip Addr - Eth1 | 172.24.193.57/255.255.255.240 |
| Ip Addr - Eth2 | 169.254.14.1/255.255.255.0 |
| Ip Addr - Eth3 | 10.10.10.1/255.255.255.0 |

# LPAR Information

|  |  |
| --- | --- |
| Lpar Name | aabasds2a |
| CPU | Desired: 10.0 | Min: 0.1 | Max: 10.0 |
| Virtual Processor | Desired: 10.0 | Min: 1.0 | Max: 10.0 |
| Memory (Gb) | Entitled: 256.0 | Min: 256.0 | Max: 256.0 |
| Power Server | AABAS2A |

|  |  |
| --- | --- |
| Lpar Name | aabasdb2a |
| CPU | Desired: 12.0 | Min: 0.1 | Max: 12.0 |
| Virtual Processor | Desired: 12.0 | Min: 1.0 | Max: 12.0 |
| Memory (Gb) | Entitled: 256.0 | Min: 256.0 | Max: 256.0 |
| Power Server | AABAS2A |

|  |  |
| --- | --- |
| Lpar Name | aabasdb2a |
| CPU | Desired: 12.0 | Min: 0.1 | Max: 12.0 |
| Virtual Processor | Desired: 12.0 | Min: 1.0 | Max: 12.0 |
| Memory (Gb) | Entitled: 256.0 | Min: 256.0 | Max: 256.0 |
| Power Server | AABAS2A |

|  |  |
| --- | --- |
| Lpar Name | VIOS2A |
| CPU | Desired: 2.0 | Min: 0.5 | Max: 2.0 |
| Virtual Processor | Desired: 2.0 | Min: 1.0 | Max: 2.0 |
| Memory (Gb) | Entitled: 32.0 | Min: 8.0 | Max: 32.0 |
| Power Server | AABAS2A |

|  |  |
| --- | --- |
| Lpar Name | aabasds2b |
| CPU | Desired: 10.0 | Min: 0.1 | Max: 10.0 |
| Virtual Processor | Desired: 10.0 | Min: 1.0 | Max: 10.0 |
| Memory (Gb) | Entitled: 256.0 | Min: 256.0 | Max: 256.0 |
| Power Server | AABAS2B |

|  |  |
| --- | --- |
| Lpar Name | aabasdb2b |
| CPU | Desired: 12.0 | Min: 0.1 | Max: 12.0 |
| Virtual Processor | Desired: 12.0 | Min: 1.0 | Max: 12.0 |
| Memory (Gb) | Entitled: 256.0 | Min: 256.0 | Max: 256.0 |
| Power Server | AABAS2B |

|  |  |
| --- | --- |
| Lpar Name | aabasdb2b |
| CPU | Desired: 12.0 | Min: 0.1 | Max: 12.0 |
| Virtual Processor | Desired: 12.0 | Min: 1.0 | Max: 12.0 |
| Memory (Gb) | Entitled: 256.0 | Min: 256.0 | Max: 256.0 |
| Power Server | AABAS2B |

|  |  |
| --- | --- |
| Lpar Name | VIOS2B |
| CPU | Desired: 1.0 | Min: 0.5 | Max: 2.0 |
| Virtual Processor | Desired: 1.0 | Min: 1.0 | Max: 2.0 |
| Memory (Gb) | Entitled: 32.0 | Min: 8.0 | Max: 32.0 |
| Power Server | AABAS2B |

|  |  |
| --- | --- |
| Lpar Name | 78-87521 |
| CPU | Desired: nan | Min: nan | Max: nan |
| Virtual Processor | Desired: nan | Min: nan | Max: nan |
| Memory (Gb) | Entitled: nan | Min: nan | Max: nan |
| Power Server | Server-9105-22B-7887521 |

# System Server Information

|  |  |
| --- | --- |
| Server Name | AABAS2A |
| Model | 9105-22A |
| Serial | 7887501 |
| CPU Cores | 24 |
| Memory (Gb) | 768 |
| Firmware Level | 01ML1060 |
| Fsp Ip Address | 172.24.193.7 |

|  |  |
| --- | --- |
| Server Name | AABAS2B |
| Model | 9105-22A |
| Serial | 7887511 |
| CPU Cores | 24 |
| Memory (Gb) | 768 |
| Firmware Level | 01ML1060 |
| Fsp Ip Address | 172.24.193.7 |

|  |  |
| --- | --- |
| Server Name | Server-9105-22B-7887521 |
| Model | 9105-22B |
| Serial | 7887521 |
| CPU Cores | 16 |
| Memory (Gb) | 320 |
| Firmware Level | 01ML1030 |
| Fsp Ip Address | 172.24.193.7 |